Endurance Bamboo

Bamboofloorin@isgn attracti e alternative to hardwoodfloors.

Naturally self-generating, "bam oo grows to maturity withinfiveyears and is regarded as the strongest


# plant on earth. nPDECK FLOORING



# Endurance Bamboo Solid Collection



Endurance Bamboo Engineered Collection

 Dimensions:

1830mm long X 190mm wide

X 3/14mm thick

Semi Gloss Finish

* Box Contains: 6 Planks = 2.0862sqm

Box Weight: 22Kg

* 5G Licensed Lock System

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| |  |  |  | | --- | --- | --- | |  |  |  | |  | Rich Brown | |  |

Proud to be a Member of the

atta

aSSOCiMian

# ENDURANCE BAMBOO SOLID COLLECTION ENDURANCE BAMBOO ENGINEERED COLLECTION TECHNICAL SPECIFICATIONS

|  |  |  |
| --- | --- | --- |
| |  | | --- | | 59 | |  |

## INSTALLATION METHOD

Floating Floor

### COATING FINISH

9 layers of Treffert water-based polyurethane finish

HARDNESS

Janka 15kn

## COLOUR COLLECTION

Lunar White, Natural, Honey Coffee, Mahogany, Forest Red, Rich Brown, French Bleed

## FIRE RATING

Critical Heat Flux & Critical Radiant Flux (CHF &

|  |
| --- |
| Combining quality & environmental control standards throughout the manufacturing process.  International  Organization for  Standardization  FSC  As bamboo is a natural product, the colour, grain and feature patterns will vary in the flooring as in the printed media.  For detail maintenance & installation guidelines please refer to the website. |

CRF) 4.9kw/m 2

## SLIP RATING

Slip Resistance Value (SRV): 15 (PI) as per Slip Resistance AS 4586 (2013)

ENVIRONMENTAL & QUALITY

## CERTIFICATES

VOC EO (0.2Mg/L) Tested in accordance to

IS016000 parts -3 -6 -9 -11 standard

IS09000 Quality control System and IS014000 Environment Control System, CE and FSC certificate

## STRUCTURAL WARRANTY

25 years residential 10 years commercial

COATING WARRANTY

5 years residential 3 years commercial